1 Firmware:
-TC-C35UN-I3-E_16MFlash_TD_EXP_NVSS_V13.6.1.20210105_filesystem.box

2 Support Product(Model & Product Number):
-TC-C35US Spec I8-A-E-Y-M-2.8~12mm(1D.20010.001195)IPC Frimware

3 Compatible Kernel Version Info: 
-NVSS_V13.6.1.20200723

4 About Fixed Bugs and Newly Added  Functions: 
-1.1 The change in the number of cutting steps corresponds to the sensor and driver
 1.2 Modify security vulnerabilities
 1.3 Solve the problem that the device cannot be logged in due to the probabilistic deadlock after the timer is turned on and restarted

5 Upgrade:
-TC-C35UN-I3-E_16MFlash_TD_EXP_NVSS_V13.6.1.20210105_filesystem.box

6 Kernel Version after Upgrading:
-NVSS_V13.6.1.20210105
